**Cisco Packet Tracer**

**Remember:**

**Console cable** = RS 232

**Changes:**

**RR** = Redirected Route

**AR** = Added Route

**Connection types:**

**FE** = FastEthernet

**GE** = GigabitEthernet

**R2 =** R 232

**Cable types:**

**CST** = Copper Straight-Through

**CCO** = Copper Cross-over

**CSL** = Console

**WL** = Wireless

**Valid connections:**

(**CST**) PC > (**FE**) > Switch1

(**CCO**) Switch1 > (**GE**) > Switch2

(**CST**) Switch2 > (**GE**) > Router1

(**RC**) (**CST**) PC > (**FE**) > Switch2

(**AR**) (**C**) PC > (**R2**) > Router1

(**WL**) Laptop > Router2